NBS Specification:



This product is associated with the following NBS Create clause:

L20 Doors/ shutters/ hatches, P30 Trenches, pipeways and pits for buried engineering services

NBS Specification:



This product is associated with the following NBS clauses:

[L20 Doors/ shutters/ hatches](https://www.ribaproductselector.com/products/doors-shutters-hatches/L20.aspx)

* [630 HATCHES](https://www.ribaproductselector.com/products/hatches/L20_630.aspx)

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/products/trenches-pipeways-and-pits-for-buried-engineering-services/P30.aspx)

* [301 ACCESS COVERS/ MANHOLE TOPS AND FRAMES](https://www.ribaproductselector.com/products/access-covers-manhole-tops-and-frames/P30_301.aspx)

Product Specification:

Kent Single Hinged Tray Fire Rated Access Cover KFRAC1000HLA

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Single Tray Fire Rated access cover

 • Type: KFRAC1000/1000(HLA)

 • Size: Manufacturer's standard – 1000mm x 1000mm clear opening

 • Load class: BS EN 124 A15 /BS EN 124 B125 /BS EN 124 C250 /BS EN 124 D400 /FACTA A /FACTA AA /FACTA AAA /FACTA B /FACTA C /FACTA D

 • Material: 1.4307 (304L) stainless steel /1.4404 (316L) stainless steel /Galvanized carbon steel

 • Tray depth: 80 mm /100 mm

 • Seal: Required (double sealed) /Not required

 • Lettering (lifting corners): Required /Not required

 • Safety barrier: Required /Not required

 • Safety grid: Required /Not required

 • Fire rating: Not required /1 h /2 h /3 h

Suggested Specification:

Kent Single Hinged Tray Fire Rated Access Cover KFRAC1000HLA

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Single Tray Fire Rated access cover

 • Type: KFRAC1000/1000(HLA)

 • Size: Manufacturer's standard – 1000mm x 1000mm clear opening

 • Load class: BS EN 124 B125

 • Material: 1.4404 (316L) stainless steel

 • Tray depth: 80 mm

 • Seal: Required (double sealed)

 • Lettering (lifting corners): Required as per project requirement

 • Safety barrier: Required

 • Safety grid: Required

 • Fire rating: 180 minutes to EN1634-1:2014