NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor gullies

NBS Specification:



This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKH215110)

* [315 FLOOR DRAINS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKH215110)

Product Specification:

KV265/110

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Industrial Gully – Side Outlet

 • Type: KV265/110 /KV265/110DS /KV365/110 /KV365/110DS /KV365/160 /KV365/160DS

 • Height: Manufacturer's standard /Bespoke

 • Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

 • Loading class to BS EN 1253: L15 /R50 /M125 /N250 /P400

 • Flange type: 4” 150lb R/F S/O ANSI Flange /4” PN10 R/F S/O Flange /Damp proof membrane flange /Holding flange /Puddle flange

 • Side inlets:

 - Type: 1½” BSP nipple /1½” BSP socket /50 mm push fit /Above ground funnel

 - Angle: 45° /90° /Bespoke

 • Grating:

 • Filter basket: Not required /Required /Required, with chain /Required, with separate filter basket

 • Accessories: None /Hinged self-sealing stainless bung

Suggested Specification:

KV265/110

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Industrial Gully – Side Outlet

 • Type: KV265/11

 • Height: Manufacturer's standard

 • Material: 1.4301 (304) stainless steel

 • Loading class to BS EN 1253: M125

 • Flange type: none

 • Side inlets: none

 • Grating: KMG Kent Mesh Grating

 • Filter basket: Required

 • Accessories: None