NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/320 Covers, gratings and frames for access chambers

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Access-CoversKentSoloPaverKSP)

* [301 ACCESS COVERS/ MANHOLE TOPS AND FRAMES](https://www.ribaproductselector.com/products/access-covers-manhole-tops-and-frames/P30_301.aspx)

Product Specification:

Kent Slot Drain Recessed Access Cover

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Solo Paver KSP

• Type: KSDRAC300/200/100(NS) / KSDRAC300/200/100(SS) / KSDRAC300/200/100(CS)

• Size: Bespoke /Manufacturer's standard

• Load class: BS EN 124 A15 /BS EN 124 B125 /BS EN 124 C250 /BS EN 124 D400 /FACTA A /FACTA AA /FACTA AAA /FACTA B /FACTA C /FACTA D

• Material:

- Type: 1.4307 (304L) stainless steel /1.4404 (316L) stainless steel /Galvanized carbon steel

- Thickness: Not applicable /3 mm /4 mm /6 mm /8 mm

• Tray depth: 80 mm /100 mm

• Seal: Required (double sealed) /Not required

• Beam pockets: Not required /Recessed /Vertical wall mounted

• Lettering (lifting corners): Required /Not required

Product Specification:

Kent Slot Drain Recessed Access Cover

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Solo Paver KSP

• Type: KSDRAC300/200/100(NS)

• Size: Manufacturer's standard

• Load class: BS EN 124 B125

- Type: 1.4404 (316L) stainless steel /Galvanized carbon steel

• Tray depth: 80 mm

• Seal: Not required

• Lettering Not required