NBS Specification:



This product is associated with the following NBS Create clause:

45-20-62/350 Tactile paving studs

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[Q25 Slab/ brick/ sett/ cobble pavings](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureStudsKentRoadDemarcationStud)

* [320 TACTILE FLAGS AND SLABS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureStudsKentRoadDemarcationStud)

Product Specification:

Kent Diamond Tactile Warning Stud

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377/+353 (0) 53 914 3216

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Diamond Tactile Warning Stud (KDTWS/35/5/FDG)

• Dimensions: 35mm diameter, 5mm top plate, 15mm stud